Phil - Probably the Vertext test command needs an argument. Otherwise it can only be used when

all three systems are available. After Luis fixes something in the Gregorian drive system, he'll phone the operator to run the test on the Greg, "Vertest G" with the syntaxt below. Jon

Vertex System Test Program?

Type "Vertest"

Prompt appears: " Az?, Greg?, Carriagehouse?, or Todos?" (all case insensitive)

Enter "T" for todos, etc

Prompt appears "hit any key to abort test"

Program then

1. Brings up power for the selected system(s) and reports any errors.

2. Moves to nearby set point. Reports if the move fails.

3. Moves back in rate mode. Reports if rate wrong.

4. Executes a track sequence. Reports if rms error too great.

5. Moves to starting point and leaves system in its original state.